2) EMERGENCY MANOEUVRE (Fig. 1)

In the case of power failure or operation malfunctions, manual emergency

manoeuvre can be carried out by turning the external release knob with

personalised key.

First turn the key clockwise, then rotate the release knob to free the gate.

The knob is to be rotated anticlockwise in the case of a left-hand leaf,

clockwise in the case of a right-hand leaf.

Keep the knob in its release position by turning the key further. Push the leaf

slowly to open or close the gate.

To reactivate motor-driven operation, free the knob from its release position

and bring it back to its initial position for normal operation.

